ep9301_hal17_2.4.21-rmk1-crus1.4.2
==================================

    2005-02-22 Michael Neuhauser <mike@firmix.at>

    Supports Cirrus EDB9301 development board with EP9301 CPU (ARM920T)
	-> http://www.cirrus.com/en/products/EDB9301_offer.html
    Might also work (with a little tweaking) with TS-7200 board from
    Technologic Systems
	-> http://www.embeddedarm.com/epc/ts7200-spec-h.html
    needs gcc >= 3.1 (3.3.2 was used during development)
    Patch chain:
    	* base is vanilla Linux 2.4.21
	    -> http://kernel.org/pub/linux/kernel/v2.4/linux-2.4.21.tar.bz2
	* apply Russel M. King's patch for this kernel:
	    patch-2.4.21-rmk1
	    -> http://www.arm.linux.org.uk/developer/v2.4/
	* apply non-public patch from board manufacturer:
	    linux-2.4.21-rmk1-crus1.4.2.patch
	    -> get it from your friendly neighborhood RTAI/ARM
	    maintainer (Michael Neuhauser <mike@firmix.at>)
	* apply Adeos patch:
	    ep9301_hal17_2.4.21-rmk1-crus1.4.2.patch
	    -> from here

    file history:
    2005-01-31 added to magma

pxa255_2.6.7-bk6-karo
=====================

    2005-02-22 Michael Neuhauser <mike@firmix.at>

    Supports Triton LP board with PXA255 CPU
	-> http://www.karo-electronics.de/index.php?id=15&L=1
    **********************************************
    *** Only immediate mode RTAI is supported! ***
    **********************************************
    (See ../../../../README.INSTALL for an explanation of immediate/piped mode.
    Bottom line: you have to execute "./mode-control immed" in ../../../scripts)
    Patch chain:
    	* base is vanilla Linux 2.6.7
	    -> http://kernel.org/pub/linux/kernel/v2.6/linux-2.6.7.tar.bz2
	* apply "official" kernel snapshot patch:
	    patch-2.6.7-bk6
	    -> http://www.kernel.org/pub/linux/kernel/v2.6/snapshots/old/patch-2.6.7-bk6.bz2
	* apply non-public(?) patch by board manufacturer:
	    linux-2.6.7-bk6-karo.patch
	    -> get it from your friendly neighborhood RTAI/ARM
	    maintainer (Michael Neuhauser <mike@firmix.at>)
	* apply Adeos patch:
	    pxa255_2.6.7-bk6-karo.patch
	    -> from here

    file history:
    2005-02-22 added to magma

at91_2.6.20.13
==============

    2007-09-14 Adeneo (by Gregory Clement, Alexandre Bouin)

    A patch to support the related Linux version on ARM-AT91, to be used after
    patching magma with: RTAI-magma-AT91.patch, also found in this repository.

    patch chain:
    linux-2.6.20.13-vanilla
    adeos-ipipe-2.6.20-arm-1.7-03.patch (from adeos project / http://gna.org/projects/adeos/)
    at91_2.6.20.13.patch

    file history:
    2007-09-14 added to www.rtai.org/RTAICONTRIB
    2008-08-06 renamed (hal-linux-2.6.20-arm-AT91 -> at91_hal-linux-2.6.20-arm-AT91)
    2008-08-06 added to magma
    2010-03-04 renamed (at91_hal-linux-2.6.20-arm-AT91 -> at91_2.6.20.13)

at91_2.6.20.13-at91sam9263
==========================

    2008-04-04 Adeneo (by Gregory CLEMENT and  Alexandre BOUIN)

    The base patch to support RTAI-magma-AT91 and RTAI-3.5-cv-AT91.
    This kernel patch adds additional rtai support for at91sam9263.

    patch chain:
    linux-2.6.20.13-vanilla
    adeos-ipipe-2.6.20-arm-1.7-03.patch (from adeos project / http://gna.org/projects/adeos/)
    at91_2.6.20.13.patch
    <kernel support for at91sam9263>
    at91_2.6.20.13-at91sam9263.patch

    file history:
    2008-04-04 added to www.rtai.org/RTAICONTRIB
    2008-08-06 renamed (adeos-ipipe-2.6.20-arm-AT91 -> at91_adeos-ipipe-2.6.20-arm-AT91)
    2008-08-06 added to magma
    2010-03-04 renamed (at91_adeos-ipipe-2.6.20-arm-AT91 -> at91_2.6.20.13-at91sam9263)

imxl_2.6.7
==========

    2008-08-06 Torsten Koschorrek <devel@koschorrek.com>

    Linux Kernel patch for mach-imx (iMXL).

    patch chain:
    linux-2.6.7-vanilla
    <kernel support for iMXL>
    imxl_2.6.7.patch


    file history:
    2008-08-06 added to magma
    2010-03-04 renamed (imx_2.6.7_rtai_3.2_v_1.0 -> imxl_2.6.7)
